Bushing & Sleeve of Clean Water Pump
应用：硬质合金耐腐蚀衬套广泛应用于市政、农业、医疗和食品行业。
Application：The cemented carbide busing & sleeve of clean water pump has special corrosion resistance material and widely be used in municipal, agricultural, medical and food industry. It is mainly used for axial sealing and rotation support of the clean water pump(i.e.:the sliding bearing subassembly), especially suitable to be assembled on the impeller of Multi-stage stainless steel centrifugal pump which is used for conveying water.

硬质合金精密产品具有优异的机械性能、高耐磨性和耐腐蚀性、高尺寸精度和规定的表面粗糙度等特点。我们使用金刚石砂轮和EDM对硬质合金半成品进行研磨。它们将被切割成各种部件，在复杂和恶劣的工作条件下替换金属部件，以提高效率并延长寿命。
　　我们的硬质合金精密产品主要包括轴套、密封环、螺纹喷嘴、衬套、阀芯、阀球和阀座、阀碟、非标准结构件和机械部件。
　　硬质合金精密零件主要用于潜油离心泵、潜油电泵、潜油分离器、潜油保护器、渣浆泵、潜油离心机、耐酸泵、废水处理泵、饮用水泵、PDC钻头、牙轮钻头、离心泵、随钻测量仪器MWD和LWD、垂直旋转导向和自激振荡旋转冲击钻井工具。
　　•材料的特殊设计和开发
　　•完整的生产流程——从材料制造到成品耐磨件
　　•20多年与国际油服公司的合作经验
　　•先进的设备和强大的系统安全能力
　　•全流程的质量控制
　　应用：硬质合金耐腐蚀衬套广泛应用于市政、农业、医疗和食品行业。 主要用于清水泵(即：滑动轴承组件)的轴向密封和旋转支撑，特别适合安装在输送水用的多级不锈钢离心泵的叶轮上。
　　技术水平：耐腐蚀性能和环保性优良(材质拥有国家专利技术)，材质通过了ROHS (中国质量检测中心)的安全认证及WRAS(英国水务中心BS6920:2000)的耐腐蚀性和环保检测认证。
The material has excellent corrosion resistance and environment protection character. The material of products is patented from China National Patent Bureau and has been certified by ROHS (China Quality Test Center) and WARS (Water service center of United Kingdom BS 69200:2000).
 
• Special Design and Development of Materials
• Complete Production Process – from Manufacturing of Materials to Finished Wear Parts
• Over 10 Years of Cooperative Experience with International Water Service Companies
• Advanced Equipment and Powerful Systematic Secure Capabilities
• Wide Range Quality Control